| OpenCV 5.0.0alpha Open Source Computer Vision

Loading...
Searching...
No Matches
Enumerations | Functions
Miscellaneous Image Transformations
Image Processing

## Detailed Description

## Enumerations
enum | cv::AdaptiveThresholdTypes { cv::ADAPTIVE_THRESH_MEAN_C = 0 , cv::ADAPTIVE_THRESH_GAUSSIAN_C = 1 }
enum | cv::DistanceTransformLabelTypes { cv::DIST_LABEL_CCOMP = 0 , cv::DIST_LABEL_PIXEL = 1 }
| distanceTransform algorithm flags More...
enum | cv::DistanceTransformMasks { cv::DIST_MASK_3 = 3 , cv::DIST_MASK_5 = 5 , cv::DIST_MASK_PRECISE = 0 }
| Mask size for distance transform. More...
enum | cv::DistanceTypes { cv::DIST_USER = -1 , cv::DIST_L1 = 1 , cv::DIST_L2 = 2 , cv::DIST_C = 3 , cv::DIST_L12 = 4 , cv::DIST_FAIR = 5 , cv::DIST_WELSCH = 6 , cv::DIST_HUBER = 7 }
enum | cv::FloodFillFlags { cv::FLOODFILL_FIXED_RANGE = 1 << 16 , cv::FLOODFILL_MASK_ONLY = 1 << 17 }
| floodfill algorithm flags More...
enum | cv::GrabCutClasses { cv::GC_BGD = 0 , cv::GC_FGD = 1 , cv::GC_PR_BGD = 2 , cv::GC_PR_FGD = 3 }
| class of the pixel in GrabCut algorithm More...
enum | cv::GrabCutModes { cv::GC_INIT_WITH_RECT = 0 , cv::GC_INIT_WITH_MASK = 1 , cv::GC_EVAL = 2 , cv::GC_EVAL_FREEZE_MODEL = 3 }
| GrabCut algorithm flags. More...
enum | cv::ThresholdTypes { cv::THRESH_BINARY = 0 , cv::THRESH_BINARY_INV = 1 , cv::THRESH_TRUNC = 2 , cv::THRESH_TOZERO = 3 , cv::THRESH_TOZERO_INV = 4 , cv::THRESH_MASK = 7 , cv::THRESH_OTSU = 8 , cv::THRESH_TRIANGLE = 16 }

## Functions
void | cv::adaptiveThreshold (InputArray src, OutputArray dst, double maxValue, int adaptiveMethod, int thresholdType, int blockSize, double C)
| Applies an adaptive threshold to an array.
void | cv::blendLinear (InputArray src1, InputArray src2, InputArray weights1, InputArray weights2, OutputArray dst)
void | cv::distanceTransform (InputArray src, OutputArray dst, int distanceType, int maskSize, int dstType=CV_32F)
void | cv::distanceTransform (InputArray src, OutputArray dst, OutputArray labels, int distanceType, int maskSize, int labelType=DIST_LABEL_CCOMP)
| Calculates the distance to the closest zero pixel for each pixel of the source image.
int | cv::floodFill (InputOutputArray image, InputOutputArray mask, Point seedPoint, Scalar newVal, Rect *rect=0, Scalar loDiff=Scalar(), Scalar upDiff=Scalar(), int flags=4)
| Fills a connected component with the given color.
int | cv::floodFill (InputOutputArray image, Point seedPoint, Scalar newVal, Rect *rect=0, Scalar loDiff=Scalar(), Scalar upDiff=Scalar(), int flags=4)
void | cv::integral (InputArray src, OutputArray sum, int sdepth=-1)
void | cv::integral (InputArray src, OutputArray sum, OutputArray sqsum, int sdepth=-1, int sqdepth=-1)
void | cv::integral (InputArray src, OutputArray sum, OutputArray sqsum, OutputArray tilted, int sdepth=-1, int sqdepth=-1)
| Calculates the integral of an image.
double | cv::threshold (InputArray src, OutputArray dst, double thresh, double maxval, int type)
| Applies a fixed-level threshold to each array element.

## Enumeration Type Documentation

## ◆ AdaptiveThresholdTypes

enum cv::AdaptiveThresholdTypes

`#include <opencv2/imgproc.hpp>`

adaptive threshold algorithm

See also
  adaptiveThreshold

Enumerator
ADAPTIVE_THRESH_MEAN_C Python: cv.ADAPTIVE_THRESH_MEAN_C | the threshold value \(T(x,y)\) is a mean of the \(\texttt{blockSize} \times \texttt{blockSize}\) neighborhood of \((x, y)\) minus C
ADAPTIVE_THRESH_GAUSSIAN_C Python: cv.ADAPTIVE_THRESH_GAUSSIAN_C | the threshold value \(T(x, y)\) is a weighted sum (cross-correlation with a Gaussian window) of the \(\texttt{blockSize} \times \texttt{blockSize}\) neighborhood of \((x, y)\) minus C . The default sigma (standard deviation) is used for the specified blockSize . See getGaussianKernel

## ◆ DistanceTransformLabelTypes

enum cv::DistanceTransformLabelTypes

`#include <opencv2/imgproc.hpp>`

distanceTransform algorithm flags

Enumerator
DIST_LABEL_CCOMP Python: cv.DIST_LABEL_CCOMP | each connected component of zeros in src (as well as all the non-zero pixels closest to the connected component) will be assigned the same label
DIST_LABEL_PIXEL Python: cv.DIST_LABEL_PIXEL | each zero pixel (and all the non-zero pixels closest to it) gets its own label.

## ◆ DistanceTransformMasks

enum cv::DistanceTransformMasks

`#include <opencv2/imgproc.hpp>`

Mask size for distance transform.

Enumerator
DIST_MASK_3 Python: cv.DIST_MASK_3 | mask=3
DIST_MASK_5 Python: cv.DIST_MASK_5 | mask=5
DIST_MASK_PRECISE Python: cv.DIST_MASK_PRECISE |

## ◆ DistanceTypes

enum cv::DistanceTypes

`#include <opencv2/imgproc.hpp>`

Distance types for Distance Transform and M-estimators

See also
  distanceTransform, fitLine

Enumerator
DIST_USER Python: cv.DIST_USER | User defined distance.
DIST_L1 Python: cv.DIST_L1 | distance = |x1-x2| + |y1-y2|
DIST_L2 Python: cv.DIST_L2 | the simple euclidean distance
DIST_C Python: cv.DIST_C | distance = max(|x1-x2|,|y1-y2|)
DIST_L12 Python: cv.DIST_L12 | L1-L2 metric: distance = 2(sqrt(1+x*x/2) - 1))
DIST_FAIR Python: cv.DIST_FAIR | distance = c^2(|x|/c-log(1+|x|/c)), c = 1.3998
DIST_WELSCH Python: cv.DIST_WELSCH | distance = c^2/2(1-exp(-(x/c)^2)), c = 2.9846
DIST_HUBER Python: cv.DIST_HUBER | distance = |x|<c ? x^2/2 : c(|x|-c/2), c=1.345

## ◆ FloodFillFlags

enum cv::FloodFillFlags

`#include <opencv2/imgproc.hpp>`

floodfill algorithm flags

Enumerator
FLOODFILL_FIXED_RANGE Python: cv.FLOODFILL_FIXED_RANGE | If set, the difference between the current pixel and seed pixel is considered. Otherwise, the difference between neighbor pixels is considered (that is, the range is floating).
FLOODFILL_MASK_ONLY Python: cv.FLOODFILL_MASK_ONLY | If set, the function does not change the image ( newVal is ignored), and only fills the mask with the value specified in bits 8-16 of flags as described above. This option only make sense in function variants that have the mask parameter.

## ◆ GrabCutClasses

enum cv::GrabCutClasses

`#include <opencv2/imgproc.hpp>`

class of the pixel in GrabCut algorithm

Enumerator
GC_BGD Python: cv.GC_BGD | an obvious background pixels
GC_FGD Python: cv.GC_FGD | an obvious foreground (object) pixel
GC_PR_BGD Python: cv.GC_PR_BGD | a possible background pixel
GC_PR_FGD Python: cv.GC_PR_FGD | a possible foreground pixel

## ◆ GrabCutModes

enum cv::GrabCutModes

`#include <opencv2/imgproc.hpp>`

GrabCut algorithm flags.

Enumerator
GC_INIT_WITH_RECT Python: cv.GC_INIT_WITH_RECT | The function initializes the state and the mask using the provided rectangle. After that it runs iterCount iterations of the algorithm.
GC_INIT_WITH_MASK Python: cv.GC_INIT_WITH_MASK | The function initializes the state using the provided mask. Note that GC_INIT_WITH_RECT and GC_INIT_WITH_MASK can be combined. Then, all the pixels outside of the ROI are automatically initialized with GC_BGD .
GC_EVAL Python: cv.GC_EVAL | The value means that the algorithm should just resume.
GC_EVAL_FREEZE_MODEL Python: cv.GC_EVAL_FREEZE_MODEL | The value means that the algorithm should just run the grabCut algorithm (a single iteration) with the fixed model

## ◆ ThresholdTypes

enum cv::ThresholdTypes

`#include <opencv2/imgproc.hpp>`

type of the threshold operation

Enumerator
THRESH_BINARY Python: cv.THRESH_BINARY | \[\texttt{dst} (x,y) = \fork{\texttt{maxval}}{if \(\texttt{src}(x,y) > \texttt{thresh}\)}{0}{otherwise}\]
THRESH_BINARY_INV Python: cv.THRESH_BINARY_INV | \[\texttt{dst} (x,y) = \fork{0}{if \(\texttt{src}(x,y) > \texttt{thresh}\)}{\texttt{maxval}}{otherwise}\]
THRESH_TRUNC Python: cv.THRESH_TRUNC | \[\texttt{dst} (x,y) = \fork{\texttt{threshold}}{if \(\texttt{src}(x,y) > \texttt{thresh}\)}{\texttt{src}(x,y)}{otherwise}\]
THRESH_TOZERO Python: cv.THRESH_TOZERO | \[\texttt{dst} (x,y) = \fork{\texttt{src}(x,y)}{if \(\texttt{src}(x,y) > \texttt{thresh}\)}{0}{otherwise}\]
THRESH_TOZERO_INV Python: cv.THRESH_TOZERO_INV | \[\texttt{dst} (x,y) = \fork{0}{if \(\texttt{src}(x,y) > \texttt{thresh}\)}{\texttt{src}(x,y)}{otherwise}\]
THRESH_MASK Python: cv.THRESH_MASK |
THRESH_OTSU Python: cv.THRESH_OTSU | flag, use Otsu algorithm to choose the optimal threshold value
THRESH_TRIANGLE Python: cv.THRESH_TRIANGLE | flag, use Triangle algorithm to choose the optimal threshold value

## Function Documentation

## ◆ adaptiveThreshold()

void cv::adaptiveThreshold | ( | InputArray | src,
|  | OutputArray | dst,
|  | double | maxValue,
|  | int | adaptiveMethod,
|  | int | thresholdType,
|  | int | blockSize,
|  | double | C )

Python:
| cv.adaptiveThreshold( | src, maxValue, adaptiveMethod, thresholdType, blockSize, C[, dst] | ) -> | dst

`#include <opencv2/imgproc.hpp>`

Applies an adaptive threshold to an array.

The function transforms a grayscale image to a binary image according to the formulae:

- THRESH_BINARY

  \[dst(x,y) = \fork{\texttt{maxValue}}{if \(src(x,y) > T(x,y)\)}{0}{otherwise}\]

- THRESH_BINARY_INV

  \[dst(x,y) = \fork{0}{if \(src(x,y) > T(x,y)\)}{\texttt{maxValue}}{otherwise}\]

  where \(T(x,y)\) is a threshold calculated individually for each pixel (see adaptiveMethod parameter).

The function can process the image in-place.

Parameters

  src | Source 8-bit single-channel image.
  dst | Destination image of the same size and the same type as src.
  maxValue | Non-zero value assigned to the pixels for which the condition is satisfied
  adaptiveMethod | Adaptive thresholding algorithm to use, see AdaptiveThresholdTypes. The BORDER_REPLICATE | BORDER_ISOLATED is used to process boundaries.
  thresholdType | Thresholding type that must be either THRESH_BINARY or THRESH_BINARY_INV, see ThresholdTypes.
  blockSize | Size of a pixel neighborhood that is used to calculate a threshold value for the pixel: 3, 5, 7, and so on.
  C | Constant subtracted from the mean or weighted mean (see the details below). Normally, it is positive but may be zero or negative as well.

See also
  threshold, blur, GaussianBlur

## ◆ blendLinear()

void cv::blendLinear | ( | InputArray | src1,
|  | InputArray | src2,
|  | InputArray | weights1,
|  | InputArray | weights2,
|  | OutputArray | dst )

Python:
| cv.blendLinear( | src1, src2, weights1, weights2[, dst] | ) -> | dst

`#include <opencv2/imgproc.hpp>`

Performs linear blending of two images:

\[ \texttt{dst}(i,j) = \texttt{weights1}(i,j)*\texttt{src1}(i,j) + \texttt{weights2}(i,j)*\texttt{src2}(i,j) \]

Parameters

  src1 | It has a type of CV_8UC(n) or CV_32FC(n), where n is a positive integer.
  src2 | It has the same type and size as src1.
  weights1 | It has a type of CV_32FC1 and the same size with src1.
  weights2 | It has a type of CV_32FC1 and the same size with src1.
  dst | It is created if it does not have the same size and type with src1.

## ◆ distanceTransform() [1/2]

void cv::distanceTransform | ( | InputArray | src,
|  | OutputArray | dst,
|  | int | distanceType,
|  | int | maskSize,
|  | int | dstType = CV_32F )

Python:
| cv.distanceTransform( | src, distanceType, maskSize[, dst[, dstType]] | ) -> | dst
| cv.distanceTransformWithLabels( | src, distanceType, maskSize[, dst[, labels[, labelType]]] | ) -> | dst, labels

`#include <opencv2/imgproc.hpp>`

This is an overloaded member function, provided for convenience. It differs from the above function only in what argument(s) it accepts.

Parameters

  src | 8-bit, single-channel (binary) source image.
  dst | Output image with calculated distances. It is a 8-bit or 32-bit floating-point, single-channel image of the same size as src .
  distanceType | Type of distance, see DistanceTypes
  maskSize | Size of the distance transform mask, see DistanceTransformMasks. In case of the DIST_L1 or DIST_C distance type, the parameter is forced to 3 because a \(3\times 3\) mask gives the same result as \(5\times 5\) or any larger aperture.
  dstType | Type of output image. It can be CV_8U or CV_32F. Type CV_8U can be used only for the first variant of the function and distanceType == DIST_L1.

## ◆ distanceTransform() [2/2]

void cv::distanceTransform | ( | InputArray | src,
|  | OutputArray | dst,
|  | OutputArray | labels,
|  | int | distanceType,
|  | int | maskSize,
|  | int | labelType = DIST_LABEL_CCOMP )

Python:
| cv.distanceTransform( | src, distanceType, maskSize[, dst[, dstType]] | ) -> | dst
| cv.distanceTransformWithLabels( | src, distanceType, maskSize[, dst[, labels[, labelType]]] | ) -> | dst, labels

`#include <opencv2/imgproc.hpp>`

Calculates the distance to the closest zero pixel for each pixel of the source image.

The function cv::distanceTransform calculates the approximate or precise distance from every binary image pixel to the nearest zero pixel. For zero image pixels, the distance will obviously be zero.

When maskSize == DIST_MASK_PRECISE and distanceType == DIST_L2 , the function runs the algorithm described in [85] . This algorithm is parallelized with the TBB library.

In other cases, the algorithm [34] is used. This means that for a pixel the function finds the shortest path to the nearest zero pixel consisting of basic shifts: horizontal, vertical, diagonal, or knight's move (the latest is available for a \(5\times 5\) mask). The overall distance is calculated as a sum of these basic distances. Since the distance function should be symmetric, all of the horizontal and vertical shifts must have the same cost (denoted as a ), all the diagonal shifts must have the same cost (denoted as `b`), and all knight's moves must have the same cost (denoted as `c`). For the DIST_C and DIST_L1 types, the distance is calculated precisely, whereas for DIST_L2 (Euclidean distance) the distance can be calculated only with a relative error (a \(5\times 5\) mask gives more accurate results). For `a`,`b`, and `c`, OpenCV uses the values suggested in the original paper:

- DIST_L1: `a = 1, b = 2`
- DIST_L2:
  - `3 x 3`: `a=0.955, b=1.3693`
  - `5 x 5`: `a=1, b=1.4, c=2.1969`
- DIST_C: `a = 1, b = 1`

Typically, for a fast, coarse distance estimation DIST_L2, a \(3\times 3\) mask is used. For a more accurate distance estimation DIST_L2, a \(5\times 5\) mask or the precise algorithm is used. Note that both the precise and the approximate algorithms are linear on the number of pixels.

This variant of the function does not only compute the minimum distance for each pixel \((x, y)\) but also identifies the nearest connected component consisting of zero pixels (labelType==DIST_LABEL_CCOMP) or the nearest zero pixel (labelType==DIST_LABEL_PIXEL). Index of the component/pixel is stored in `labels(x, y)`. When labelType==DIST_LABEL_CCOMP, the function automatically finds connected components of zero pixels in the input image and marks them with distinct labels. When labelType==DIST_LABEL_PIXEL, the function scans through the input image and marks all the zero pixels with distinct labels.

In this mode, the complexity is still linear. That is, the function provides a very fast way to compute the Voronoi diagram for a binary image. Currently, the second variant can use only the approximate distance transform algorithm, i.e. maskSize=DIST_MASK_PRECISE is not supported yet.

Parameters

  src | 8-bit, single-channel (binary) source image.
  dst | Output image with calculated distances. It is a 8-bit or 32-bit floating-point, single-channel image of the same size as src.
  labels | Output 2D array of labels (the discrete Voronoi diagram). It has the type CV_32SC1 and the same size as src.
  distanceType | Type of distance, see DistanceTypes
  maskSize | Size of the distance transform mask, see DistanceTransformMasks. DIST_MASK_PRECISE is not supported by this variant. In case of the DIST_L1 or DIST_C distance type, the parameter is forced to 3 because a \(3\times 3\) mask gives the same result as \(5\times 5\) or any larger aperture.
  labelType | Type of the label array to build, see DistanceTransformLabelTypes.

## ◆ floodFill() [1/2]

int cv::floodFill | ( | InputOutputArray | image,
|  | InputOutputArray | mask,
|  | Point | seedPoint,
|  | Scalar | newVal,
|  | Rect * | rect = 0,
|  | Scalar | loDiff = Scalar(),
|  | Scalar | upDiff = Scalar(),
|  | int | flags = 4 )

Python:
| cv.floodFill( | image, mask, seedPoint, newVal[, loDiff[, upDiff[, flags]]] | ) -> | retval, image, mask, rect

`#include <opencv2/imgproc.hpp>`

Fills a connected component with the given color.

The function cv::floodFill fills a connected component starting from the seed point with the specified color. The connectivity is determined by the color/brightness closeness of the neighbor pixels. The pixel at \((x,y)\) is considered to belong to the repainted domain if:

- in case of a grayscale image and floating range

  \[\texttt{src} (x',y')- \texttt{loDiff} \leq \texttt{src} (x,y) \leq \texttt{src} (x',y')+ \texttt{upDiff}\]

- in case of a grayscale image and fixed range

  \[\texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)- \texttt{loDiff} \leq \texttt{src} (x,y) \leq \texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)+ \texttt{upDiff}\]

- in case of a color image and floating range

  \[\texttt{src} (x',y')_r- \texttt{loDiff} _r \leq \texttt{src} (x,y)_r \leq \texttt{src} (x',y')_r+ \texttt{upDiff} _r,\]

  \[\texttt{src} (x',y')_g- \texttt{loDiff} _g \leq \texttt{src} (x,y)_g \leq \texttt{src} (x',y')_g+ \texttt{upDiff} _g\]

  and

  \[\texttt{src} (x',y')_b- \texttt{loDiff} _b \leq \texttt{src} (x,y)_b \leq \texttt{src} (x',y')_b+ \texttt{upDiff} _b\]

- in case of a color image and fixed range

  \[\texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)_r- \texttt{loDiff} _r \leq \texttt{src} (x,y)_r \leq \texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)_r+ \texttt{upDiff} _r,\]

  \[\texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)_g- \texttt{loDiff} _g \leq \texttt{src} (x,y)_g \leq \texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)_g+ \texttt{upDiff} _g\]

  and

  \[\texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)_b- \texttt{loDiff} _b \leq \texttt{src} (x,y)_b \leq \texttt{src} ( \texttt{seedPoint} .x, \texttt{seedPoint} .y)_b+ \texttt{upDiff} _b\]

where \(src(x',y')\) is the value of one of pixel neighbors that is already known to belong to the component. That is, to be added to the connected component, a color/brightness of the pixel should be close enough to:

- Color/brightness of one of its neighbors that already belong to the connected component in case of a floating range.
- Color/brightness of the seed point in case of a fixed range.

Use these functions to either mark a connected component with the specified color in-place, or build a mask and then extract the contour, or copy the region to another image, and so on.

Parameters

  image | Input/output 1- or 3-channel, 8-bit, or floating-point image. It is modified by the function unless the FLOODFILL_MASK_ONLY flag is set in the second variant of the function. See the details below.
  mask | Operation mask that should be a single-channel 8-bit image, 2 pixels wider and 2 pixels taller than image. If an empty Mat is passed it will be created automatically. Since this is both an input and output parameter, you must take responsibility of initializing it. Flood-filling cannot go across non-zero pixels in the input mask. For example, an edge detector output can be used as a mask to stop filling at edges. On output, pixels in the mask corresponding to filled pixels in the image are set to 1 or to the specified value in flags as described below. Additionally, the function fills the border of the mask with ones to simplify internal processing. It is therefore possible to use the same mask in multiple calls to the function to make sure the filled areas do not overlap.
  seedPoint | Starting point.
  newVal | New value of the repainted domain pixels.
  loDiff | Maximal lower brightness/color difference between the currently observed pixel and one of its neighbors belonging to the component, or a seed pixel being added to the component.
  upDiff | Maximal upper brightness/color difference between the currently observed pixel and one of its neighbors belonging to the component, or a seed pixel being added to the component.
  rect | Optional output parameter set by the function to the minimum bounding rectangle of the repainted domain.
  flags | Operation flags. The first 8 bits contain a connectivity value. The default value of 4 means that only the four nearest neighbor pixels (those that share an edge) are considered. A connectivity value of 8 means that the eight nearest neighbor pixels (those that share a corner) will be considered. The next 8 bits (8-16) contain a value between 1 and 255 with which to fill the mask (the default value is 1). For example, 4 | ( 255 << 8 ) will consider 4 nearest neighbours and fill the mask with a value of 255. The following additional options occupy higher bits and therefore may be further combined with the connectivity and mask fill values using bit-wise or (|), see FloodFillFlags.

Note
  Since the mask is larger than the filled image, a pixel \((x, y)\) in image corresponds to the pixel \((x+1, y+1)\) in the mask .

See also
  findContours

## ◆ floodFill() [2/2]

int cv::floodFill | ( | InputOutputArray | image,
|  | Point | seedPoint,
|  | Scalar | newVal,
|  | Rect * | rect = 0,
|  | Scalar | loDiff = Scalar(),
|  | Scalar | upDiff = Scalar(),
|  | int | flags = 4 )

Python:
| cv.floodFill( | image, mask, seedPoint, newVal[, loDiff[, upDiff[, flags]]] | ) -> | retval, image, mask, rect

`#include <opencv2/imgproc.hpp>`

This is an overloaded member function, provided for convenience. It differs from the above function only in what argument(s) it accepts.

variant without `mask` parameter

## ◆ integral() [1/3]

void cv::integral | ( | InputArray | src,
|  | OutputArray | sum,
|  | int | sdepth = -1 )

Python:
| cv.integral( | src[, sum[, sdepth]] | ) -> | sum
| cv.integral2( | src[, sum[, sqsum[, sdepth[, sqdepth]]]] | ) -> | sum, sqsum
| cv.integral3( | src[, sum[, sqsum[, tilted[, sdepth[, sqdepth]]]]] | ) -> | sum, sqsum, tilted

`#include <opencv2/imgproc.hpp>`

This is an overloaded member function, provided for convenience. It differs from the above function only in what argument(s) it accepts.

## ◆ integral() [2/3]

void cv::integral | ( | InputArray | src,
|  | OutputArray | sum,
|  | OutputArray | sqsum,
|  | int | sdepth = -1,
|  | int | sqdepth = -1 )

Python:
| cv.integral( | src[, sum[, sdepth]] | ) -> | sum
| cv.integral2( | src[, sum[, sqsum[, sdepth[, sqdepth]]]] | ) -> | sum, sqsum
| cv.integral3( | src[, sum[, sqsum[, tilted[, sdepth[, sqdepth]]]]] | ) -> | sum, sqsum, tilted

`#include <opencv2/imgproc.hpp>`

This is an overloaded member function, provided for convenience. It differs from the above function only in what argument(s) it accepts.

## ◆ integral() [3/3]

void cv::integral | ( | InputArray | src,
|  | OutputArray | sum,
|  | OutputArray | sqsum,
|  | OutputArray | tilted,
|  | int | sdepth = -1,
|  | int | sqdepth = -1 )

Python:
| cv.integral( | src[, sum[, sdepth]] | ) -> | sum
| cv.integral2( | src[, sum[, sqsum[, sdepth[, sqdepth]]]] | ) -> | sum, sqsum
| cv.integral3( | src[, sum[, sqsum[, tilted[, sdepth[, sqdepth]]]]] | ) -> | sum, sqsum, tilted

`#include <opencv2/imgproc.hpp>`

Calculates the integral of an image.

The function calculates one or more integral images for the source image as follows:

\[\texttt{sum} (X,Y) = \sum _{x<X,y<Y} \texttt{image} (x,y)\]

\[\texttt{sqsum} (X,Y) = \sum _{x<X,y<Y} \texttt{image} (x,y)^2\]

\[\texttt{tilted} (X,Y) = \sum _{y<Y,abs(x-X+1) \leq Y-y-1} \texttt{image} (x,y)\]

Using these integral images, you can calculate sum, mean, and standard deviation over a specific up-right or rotated rectangular region of the image in a constant time, for example:

\[\sum _{x_1 \leq x < x_2, \, y_1 \leq y < y_2} \texttt{image} (x,y) = \texttt{sum} (x_2,y_2)- \texttt{sum} (x_1,y_2)- \texttt{sum} (x_2,y_1)+ \texttt{sum} (x_1,y_1)\]

It makes possible to do a fast blurring or fast block correlation with a variable window size, for example. In case of multi-channel images, sums for each channel are accumulated independently.

As a practical example, the next figure shows the calculation of the integral of a straight rectangle Rect(4,4,3,2) and of a tilted rectangle Rect(5,1,2,3) . The selected pixels in the original image are shown, as well as the relative pixels in the integral images sum and tilted .

integral calculation example

Parameters

  src | input image as \(W \times H\), 8-bit or floating-point (32f or 64f).
  sum | integral image as \((W+1)\times (H+1)\) , 32-bit integer or floating-point (32f or 64f).
  sqsum | integral image for squared pixel values; it is \((W+1)\times (H+1)\), double-precision floating-point (64f) array.
  tilted | integral for the image rotated by 45 degrees; it is \((W+1)\times (H+1)\) array with the same data type as sum.
  sdepth | desired depth of the integral and the tilted integral images, CV_32S, CV_32F, or CV_64F.
  sqdepth | desired depth of the integral image of squared pixel values, CV_32F or CV_64F.

## ◆ threshold()

double cv::threshold | ( | InputArray | src,
|  | OutputArray | dst,
|  | double | thresh,
|  | double | maxval,
|  | int | type )

Python:
| cv.threshold( | src, thresh, maxval, type[, dst] | ) -> | retval, dst

`#include <opencv2/imgproc.hpp>`

Applies a fixed-level threshold to each array element.

The function applies fixed-level thresholding to a multiple-channel array. The function is typically used to get a bi-level (binary) image out of a grayscale image ( compare could be also used for this purpose) or for removing a noise, that is, filtering out pixels with too small or too large values. There are several types of thresholding supported by the function. They are determined by type parameter.

Also, the special values THRESH_OTSU or THRESH_TRIANGLE may be combined with one of the above values. In these cases, the function determines the optimal threshold value using the Otsu's or Triangle algorithm and uses it instead of the specified thresh.

Note
  Currently, the Otsu's and Triangle methods are implemented only for 8-bit single-channel images.

Parameters

  src | input array (multiple-channel, 8-bit or 32-bit floating point).
  dst | output array of the same size and type and the same number of channels as src.
  thresh | threshold value.
  maxval | maximum value to use with the THRESH_BINARY and THRESH_BINARY_INV thresholding types.
  type | thresholding type (see ThresholdTypes).

Returns
  the computed threshold value if Otsu's or Triangle methods used.

See also
  adaptiveThreshold, findContours, compare, min, max