| OpenCV 3.4.1 Open Source Computer Vision

Functions
Autocalibration
Images stitching

## Functions
bool | cv::detail::calibrateRotatingCamera (const std::vector< Mat > &Hs, Mat &K)
void | cv::detail::estimateFocal (const std::vector< ImageFeatures > &features, const std::vector< MatchesInfo > &pairwise_matches, std::vector< double > &focals)
| Estimates focal lengths for each given camera. More...
void | cv::detail::focalsFromHomography (const Mat &H, double &f0, double &f1, bool &f0_ok, bool &f1_ok)
| Tries to estimate focal lengths from the given homography under the assumption that the camera undergoes rotations around its centre only. More...

## Detailed Description

## Function Documentation

## § calibrateRotatingCamera()

bool cv::detail::calibrateRotatingCamera | ( | const std::vector< Mat > & | Hs,
|  | Mat & | K
| ) |  |

## § estimateFocal()

void cv::detail::estimateFocal | ( | const std::vector< ImageFeatures > & | features,
|  | const std::vector< MatchesInfo > & | pairwise_matches,
|  | std::vector< double > & | focals
| ) |  |

Estimates focal lengths for each given camera.

Parameters

  features | Features of images.
  pairwise_matches | Matches between all image pairs.
  focals | Estimated focal lengths for each camera.

## § focalsFromHomography()

void cv::detail::focalsFromHomography | ( | const Mat & | H,
|  | double & | f0,
|  | double & | f1,
|  | bool & | f0_ok,
|  | bool & | f1_ok
| ) |  |

Tries to estimate focal lengths from the given homography under the assumption that the camera undergoes rotations around its centre only.

Parameters

  H | Homography.
  f0 | Estimated focal length along X axis.
  f1 | Estimated focal length along Y axis.
  f0_ok | True, if f0 was estimated successfully, false otherwise.
  f1_ok | True, if f1 was estimated successfully, false otherwise.

See "Construction of Panoramic Image Mosaics with Global and Local Alignment" by Heung-Yeung Shum and Richard Szeliski.