| OpenCV 5.0.0alpha Open Source Computer Vision

Loading...
Searching...
No Matches
Typedefs
simd512 Namespace Reference

## Typedefs
typedef v_float32x16 | v_float32
| Maximum available vector register capacity 32-bit floating point values (single precision)
typedef v_float64x8 | v_float64
| Maximum available vector register capacity 64-bit floating point values (double precision)
typedef v_int16x32 | v_int16
| Maximum available vector register capacity 16-bit signed integer values.
typedef v_int32x16 | v_int32
| Maximum available vector register capacity 32-bit signed integer values.
typedef v_int64x8 | v_int64
| Maximum available vector register capacity 64-bit signed integer values.
typedef v_int8x64 | v_int8
| Maximum available vector register capacity 8-bit signed integer values.
typedef v_uint16x32 | v_uint16
| Maximum available vector register capacity 16-bit unsigned integer values.
typedef v_uint32x16 | v_uint32
| Maximum available vector register capacity 32-bit unsigned integer values.
typedef v_uint64x8 | v_uint64
| Maximum available vector register capacity 64-bit unsigned integer values.
typedef v_uint8x64 | v_uint8
| Maximum available vector register capacity 8-bit unsigned integer values.